For 1990-2009 cars

### Removal Procedure

1. Remove the windshield wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer System.
2. Remove the following components from the vehicle:

• | The 5 screws

• | The 6 plastic retainers

• | The air inlet grille panel (1)

3. Remove the rear hood seal from the air inlet grille panel, if necessary. Refer to Hood Rear Seal Replacement .

### Installation Procedure

1. Install the rear hood seal to the air inlet grille panel, if removed. Refer to Hood Rear Seal Replacement .
2. Install the air inlet grille panel (1) to the vehicle. Secure the panel with the following fasteners:

• | The 5 screws

• | The 6 plastic retainers

3. Install the windshield wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer System.