For 1990-2009 cars

### Removal Procedure

1. Gently pry the hood latch release handle (1) from the I/P drivers knee bolster trim (2).
2. Remove the hood latch release cable (1) from the hood latch release handle (2).
3. Remove the hood latch release handle (2) from the vehicle.

### Installation Procedure

1. Install the hood latch release cable (1) to the hood latch release handle (2).
2. Install the hood release latch handle (1) to the I/P drivers knee bolster trim (2).