For 1990-2009 cars

### Removal Procedure

1. Remove the rear end trim finish panels. Refer to Rear Compartment Side Trim Replacement - Left Side and Rear Compartment Side Trim Replacement - Right Side .
2. Remove the rear compartment sill trim plate. Refer to Rear Compartment Trim Panel Replacement .
3. Disconnect the rear compartment lid lamp switch (2) electrical connector.
4. Remove the following components from the vehicle:

• | The 2 bolts

• | The rear compartment lid lock striker (1)

5. Remove the following components from the lock striker:

• | The screw

• | The rear compartment lid lamp switch (2)

### Installation Procedure

1. Install the rear compartment lid lamp switch (2) to the rear compartment lid lock striker. Secure the switch with the screw.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear compartment lid lock striker (1) to vehicle. Secure the striker with the 2 bolts.

Tighten
Tighten the rear compartment lid lock striker bolts to 5 N·m (43 lb in).

3. Connect the rear compartment lid lamp switch (2) electrical connector.
4. Install the rear compartment sill trim plate. Refer to Rear Compartment Trim Panel Replacement .
5. Install the rear end trim finish panel. Refer to Rear Compartment Side Trim Replacement - Left Side and Rear Compartment Side Trim Replacement - Right Side .