For 1990-2009 cars

The condition of an automatic transaxle not operating properly may be influenced by one or a combination of the following items:

• | The fluid level may be too high or too low. Refer to Fluid Level Checking Procedures.

• | The engine may be performing poorly. Refer to Driveability and Emissions or Engine General Information and Mechanical Diagnosis.

• | The throttle valve (TV) cable may be out of adjustment. Refer to TV Cable Adjustment.

• | The shift select cable may be out of adjustment. Refer to Shift Select Cable.

• | The transaxle may have internal fluid leaks. Refer to the Transmission/Transaxle/Transfer Case Unit Repair Manual.

• | There may be a problem with the electrical system. Refer to Engine Electrical and Electrical Diagnosis in Unit Repair.

• | The vehicle may have a problem in the transaxle or in the other mechanical components. Refer to On-Vehicle Service.