For 1990-2009 cars

### Removal Procedure

1. Open the door.
2. Remove the bolt (3) that retains the rear door check link (2) to the door jamb.
3. Remove the following components from the door (2):

• | The rear door weatherstrip (1)

• | The plastic retainers

### Installation Procedure

1. Install the rear door weatherstrip (1) to the door (2). Ensure that the plastic retainers are completely engaged.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt (3) that retains the rear door check link (2) to the door jamb.

Tighten
Tighten the bolt to 5.5 N·m (49 lb in).