For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Remove the following components from the vehicle:

• | The plastic retainer

• | The 3 bolts (3)

3. Disconnect the hood latch release cable (1).
4. Remove the hood latch (2) from the vehicle.

### Installation Procedure

1. Install the hood latch release cable (1) to the hood latch (2).
2. Install the hood latch (1) to the vehicle. Secure the latch with the 3 bolts (3) and one plastic retainer but do not tighten fully.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Make the following adjustments to the hood latch:

• | The striker shaft lines up with the center groove of the latch.

• | The hood is flush with the front fender. Refer to Hood Adjustment .

Tighten
Tighten the hood latch bolts to 15 N·m (11 lb ft).

4. Lower the hood.