For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Raise and properly support the engine. Refer to Engine Support Fixture .
3. Remove the right side engine mount-to-engine bracket bolts and nuts (3).
4. Remove the three right side engine mount-to-frame bolts.
5. Raise the engine slightly in order to provide clearance for the engine mount assembly removal.
6. Remove the right side engine mount from the vehicle.
7. Remove the right side engine mount-to-frame bracket from the engine mount.
8. Remove the right side engine mount-to-engine bracket from the engine mount.

### Installation Procedure

1. Install the right side engine mount-to-engine bracket to the engine mount.
2. Install the right side engine mount-to-frame bracket to the engine mount.
3. Install the right side engine mount to the engine.
4. Install the three right side engine mount-to-frame bolts. Do not fully tighten the bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the three right side engine mount-to-engine bracket bolt and nuts.

#### Tighten

• | Tighten the right side engine mount-to-frame bolts to 54 N·m (40 lb ft).

• | Tighten the right side engine mount-to-engine bracket bolt and nuts (3) to 54 N·m (40 lb ft).

6. Remove the engine support fixture.
7. Connect the negative battery cable.

Tighten
Tighten the battery cable bolt to 15 N·m (11 lb ft).