For 1990-2009 cars

### Removal Procedure

1. Disconnect the accelerator cable from the accelerator pedal lever.
2. Remove the 2 bolts (3).
3. Remove the accelerator pedal and the pedal lever from the vehicle.
4. Remove the one retainer, the spring, the pin, and the accelerator pedal from the pedal lever.

### Installation Procedure

1. Connect the accelerator pedal to the pedal lever. Secure the pedal with one pin, a spring, and a retainer.
2. Connect the accelerator pedal and the pedal lever to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Secure with the 2 bolts (3).

Tighten
Tighten the bracket bolts to 10 N·m (89 lb in).

4. Connect the accelerator cable to the accelerator pedal lever.