For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Door Lock System Check? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 | Can the suspect door lock switch lock the door? | -- | Go to Step 3 | Go to Step 6
3 | Test for an open in the BLU/YEL wire using a J 39200 DMM from the suspected door lock switch connector. Does the wire have an open? | -- | Go to Step 5 | Go to Step 4
4 | Replace the suspected door lock switch. Is the repair complete? | -- | Go to Power Door Locks System Check | --
5 | Repair the open in the BLU/YEL wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
6 | Can the suspect door lock switch unlock the door? | -- | Go to Step 7 | Go to Step 9
7 | Test for an open in the BLU/WHT wire using a J 39200 DMM from the suspected door lock switch connector. Does the wire have an open? | -- | Go to Step 8 | Go to Step 4
8 | Repair the open in the BLU/WHT wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
9 | Test for an open in the WHT/BLK wire us a J 39200 DMM coming from the door lock switch connector. Does the wire have an open? | -- | Go to Step 10 | Go to Step 4
10 | Repair the open in the WHT/BLK wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --