For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.
2. Remove the windshield defroster nozzle duct (2) from the heater case assembly.

### Installation Procedure

1. Install the windshield defroster nozzle duct (2) to the heater case assembly.
2. Install the IP assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.