For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 | Do the headlights illuminate when turned ON? | -- | Go to Step 3 | Go to Headlight System Check
3 |

1. Using a fused jumper wire, connect the LH front door jamb switch connector lead to ground.
2. Set the conditions to activate the lights on chime.

Did the lights on chime sound?

--

Go to Step 4

Go to Step 5

4 | Repair the open in the RED/WHT wire from the junction block 2, C4 cavity 7. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
5 | Replace the LH front door jamb switch. Refer to Wiring Repairs . Is the repair complete? | -- | Go to Audible Warnings System Check | --