For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Were you sent here from the Headlight System Check? | -- | Go to Step 2 | Go to Headlight System Check
2 | Measure the voltage at the head (RH-UPR) fuse. Is the measured voltage within the specified limits? | B+ | Go to Step 3 | Go to Step 4
3 | Locate and repair the open in the RED/YEL wire between the fuse and the RH headlamp. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --
4 | Replace the fuse and relay block 1. Refer to Underhood Fuse Block Replacement in Engine Electrical. Is the replacement complete? | -- | Go to Headlight System Check | --