For 1990-2009 cars

### Removal Procedure

1. Remove the front side door sill trim plate. Refer to Door Sill Plate Replacement .
2. Remove the plastic retainer (1) which secures the center pillar lower trim panel (2).
3. Remove the center pillar lower trim panel (1) by gently prying loose.

### Installation Procedure

1. Install the center pillar lower trim panel (1) to the vehicle.
2. Secure the center pillar lower trim panel (2) with the plastic retainer (1).
3. Install the front side door sill trim plate (1) to the vehicle.