For 1990-2009 cars

### Removal Procedure

1. Remove the headlining trim finish panel. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Disconnect the sunroof actuator electrical connector.

Important: Remove the sunroof actuator with the motor in the fully closed position.

3. Remove the following components from the vehicle:

• | The 3 bolts (1)

• | The sunroof actuator (4)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the sunroof actuator (4) to the vehicle. Secure the actuator with the 3 bolts (1).

Tighten
Tighten the sunroof actuator bolts to 5.4 N·m (48 lb in).

2. Connect the sunroof actuator electrical connector.
3. Install the headlining trim finish panel. Refer to Headlining Trim Panel Replacement in Interior Trim.