For 1990-2009 cars

### Removal Procedure

1. Raise the rear compartment lid.
2. Remove the 2 bolts (1) that retain the rear compartment lid lock (2) to the rear compartment lid.
3. Remove the rear compartment lid lock cylinder rod (6) from the lock (2).
4. Remove the lock (2) from the vehicle.
5. If the vehicle is equipped with a remote rear compartment release, remove the rear compartment lid lock release cable (3) from the rear compartment lid lock (2).

### Installation Procedure

1. If the vehicle is equipped with a remote rear compartment release, install the rear compartment lid lock release cable (3) to rear compartment lid lock (2).
2. Install the rear compartment lid lock cylinder rod (6) to the lock (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rear compartment lid lock (2) to the rear compartment lid. Secure the lock with the 2 bolts (1).

Tighten
Tighten the rear compartment lid lock bolts to 5 N·m (43 lb in).

4. Lower the rear compartment lid.