For 1990-2009 cars

Periodically inspect all of the following components:

• | The brake pipes

• | The hoses

• | The connections

Perform the inspection during an engine oil change. Use a light and mirror for an adequate inspection.

1. Inspect the hydraulic brake pipe and hoses for the following conditions:

• | Road hazard damage

• | Cracks and chafing of the outer cover of the brake hoses

• | Leaks and blisters

• | Proper routing and mounting

• | Damage, cracks, dents and corrosion on the brake pipe

• | If any of these conditions are discovered, replace the affected brake pipe or hose.

2. Inspect the brake pipe and the brake hose connections for leaks. If a leak is found, complete the following steps:

• | Verify the torque of the fasteners.

• | Replace the pipe or the hose.