For 1990-2009 cars

### Removal Procedure

1. Remove the screw and gently pry the bezel (2) from the courtesy and reading lamp/sunroof switch assembly (1).
2. Remove the screw which secures the courtesy and reading lamp/sunroof switch assembly (1) to the roof.
3. Disconnect the courtesy and reading lamp/sunroof switch assembly electrical connector.
4. Remove the courtesy and reading lamp/sunroof switch assembly (1) from the vehicle.

### Installation Procedure

1. Connect the courtesy and reading lamp/sunroof switch assembly electrical connector.
2. Install the courtesy and reading lamp/sunroof switch assembly (1) to the roof. Secure the switch assembly with the screw.
3. Install the bezel (2) to the courtesy and reading lamp/sunroof switch assembly (1). Secure the bezel with the screw.