For 1990-2009 cars

### Description

Several states require that a vehicle pass on-board diagnostic (OBD) system tests and the I/M emission inspection in order to renew license plates. This is accomplished by viewing the I/M System Status display on a scan tool. Using a scan tool, the technician can observe the I/M System Status in order to verify that the vehicle meets the criteria that complies with the local area requirements.

### Conditions for Updating the I/M System Status

Each system requires at least one, and sometimes several, diagnostic tests. The results of these tests are reported by a diagnostic trouble code (DTC). A system monitor is complete when either all of the DTCs comprising the monitor have Run and Passed, or any one of the DTCs comprising the monitor have illuminated the malfunction indicator lamp (MIL). Once all of the tests are completed, the I/M System Status display will indicate YES in the Completed column. For example, when the HO2S Heater Test indicates YES, all of the oxygen sensor heaters have been diagnosed. If the vehicle has four heated oxygen sensors, all four heater circuits have been diagnosed. The I/M System Status will indicate NO under the Completed column when any of the required tests for that system have not run. The following is a list of conditions that would set the I/M System Status indicator to NO:

• | The vehicle is new from the factory and has not yet been driven through the necessary drive conditions to complete the tests.

• | The battery has been disconnected or discharged below operating voltage.

• | The control module power or ground has been interrupted.

• | The control module has been reprogrammed.

• | The control module DTCs have been cleared as part of a service procedure.

### Monitored Emission Control Systems

The OBD II system monitors all emission control systems that are on-board. Not all vehicles have a full complement of emission control systems. For example, a vehicle may not be equipped with secondary air injection (AIR) or exhaust gas recirculation (EGR). The OBD II regulations require monitoring of the following:

• | Air conditioning system

• | Catalytic converter efficiency

• | Comprehensive component monitoring -- Emission related inputs and outputs

• | Evaporative emissions (EVAP) system

• | Exhaust gas recirculation (EGR) system

• | Fuel delivery system

• | Heated catalyst monitoring

• | Misfire monitoring

• | Oxygen sensor system (O2S or HO2S)

• | Oxygen sensor heater system (HO2S heater)

• | Secondary air injection (AIR) system

For the specific DTCs required for each system, refer to Inspection/Maintenance (I/M) System DTC Table . Systems such as fuel delivery, misfire, and comprehensive components may not be listed in a system status list. These tests run continuously on some vehicles and may not require an indicator.

### Diagnostic Aids

The I/M System Status display provides an indication of when the control module has completed the required tests. This does not necessarily mean that the test has passed, only that a decision was made. If the diagnostic fails, a DTC will indicate the failure. If a failure indication is present for a DTC associated with one of the I/M regulated systems, the DTC may prevent other required tests from running. For example, a DTC for the control circuit of the relay controlling an AIR pump may not be listed in the Inspection/Maintenance System DTC Table because the DTC is a continuous test. If this DTC is set, the Active Tests for the AIR system may not run.

The I/M System Status information may be useful for a technician to determine if diagnostics have run when verifying repairs.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Any DTCs set, even those that are not listed in the Inspection/Maintenance System DTC Table, may prevent the required DTCs from running. If there is any question as to whether a set DTC is disabling the required I/M diagnostic, review the Conditions for Running in the diagnostic procedures for the DTC required by the I/M diagnostic. A list of disabling DTCs, if applicable, is contained in the supporting text for that DTC.

2. Anytime a control module is reprogrammed or the diagnostic trouble codes are cleared as part of a repair procedure, all the I/M System Status indicators will reset to NO.

3. Use discretion when determining whether the entire system set procedure needs to be performed. For example, if the only tests that have not run are those that require the engine to be at operating temperature, then only those individual tests need to be run. There is no need to allow the engine to completely cool in order to run these tests.

Step | Action | Yes | No
--- | --- | --- | ---
1 |

1. Perform Diagnostic System Check - Engine Controls .

Important: Many DTC related repairs will instruct the technician to clear the DTC information. This procedure will reset ALL of the I/M System Status indicators to NO, and require performing the I/M Complete System Set Procedure.

2. Repair any DTCs or driveability concerns that would prevent the I/M System Status tests from completing.

Did you find and repair a DTC or driveability concern?

Go to Step 3

Go to Step 2

2 |

1. Review any service bulletins for software updates that may prevent I/M readiness.
2. Perform any repairs indicated by the service bulletins.

Was a repair service required?

Go to Inspection/Maintenance (I/M) Complete System Set Procedure

Go to Step 3

3 | With a scan tool, observe the I/M System Status display. Is more than one test indicating a NO status? | Go to Inspection/Maintenance (I/M) Complete System Set Procedure | Go to the I/M System Set Procedure for the indicated system