For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Panel Replacement .
2. Straighten the retaining tabs (3) and remove the inner sealing strip (1) from the front door trim panel (2).

### Installation Procedure

1. Install the inner sealing strip (1) to the front door trim panel (2). Bend the retaining tabs (3) in order to secure the inner sealing strip (1).
2. Install the front side door trim. Refer to Front Side Door Trim Panel Replacement .