For 1990-2009 cars

## Air Distributor Duct Replacement Left

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.
2. Remove the following components from the IP assembly:

• | The plastic retainer (1)

• | The left IP outer air outlet duct (2)

### Installation Procedure

1. Install the left IP outer air outlet duct (2) to the IP assembly. Secure the duct with the plastic retainer (1).
2. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gages and Console.

## Air Distributor Duct Replacement Right

### Removal Procedure

1. Remove the instrument panel (IP) assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.
2. Remove the following components from the IP:

• | The 1 screw

• | The right IP outer air outlet duct (3)

### Installation Procedure

1. Install the right IP outer air outlet duct (3) to the IP. Secure the duct with the screw.
2. Install the IP assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.