For 1990-2009 cars

## Clutch Rotor and Bearing Removal V5 - Direct Mount

#### Tools Required

• | J 41790-A Compressor Holding Fixture

• | J 41552 Compressor Pulley Puller

• | J 33023-A Puller Pilot

1. Install the compressor onto the J 41790-A .
2. Remove the clutch plate and hub assembly (2).
3. Remove the clutch rotor and bearing assembly retaining ring (3), using external snap ring pliers (1).
4. Place the J 33023-A on the clutch rotor.
5. Install the J 41552 down into the inner circle of slots in the rotor.

Turn the compressor pulley puller clockwise in the slots to engage the puller tangs with the rotor.

6. Hold the compressor pulley puller in place and use a wrench to turn the center forcing screw against the puller pilot to remove the clutch rotor and bearing assembly.