For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .
2. Straighten the retaining tabs (3) and remove the inner sealing strip (1) from the rear door trim panel (2).

### Installation Procedure

1. Install the inner sealing strip (1) to the trim panel (2). Bend the retaining tabs (3) in order to secure the inner sealing strip (1).
2. Install the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .