For 1990-2009 cars

### Removal Procedure

1. Fold the rear seat back cushion to the down position.
2. Remove the 2 plastic carpet retainers which secure the back of the seat back cushion cover to the rear compartment area.
3. Remove the outer pivot support bolt (2) from the rear seat back cushion (1).
4. Remove the following components from the vehicle:

• | The center pivot support bolt (2)

• | The rear seat back cushion (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear seat back cushion (1) to the vehicle. Secure the rear seat back cushion with the center pivot support bolt (2).

Tighten
Tighten the center pivot support bolt to 18 N·m (13 lb ft).

2. Install the outer pivot support bolt (2) to the rear seat back cushion (1).

Tighten
Tighten the outer pivot support bolt to 18 N·m (13 lb ft).

3. Install the 2 plastic carpet retainers which secure the back of the seat back cushion cover to the rear compartment area.
4. Return the seat back to the upright position.