For 1990-2009 cars

The proportioning valve is located on the vehicle cowl behind the engine.

The proportioning valve limits the outlet pressure to the rear brakes after a predetermined master cylinder pressure is reached. This feature is used when less rear apply force is needed. This feature performs the following functions:

• | Allows smooth braking action

• | Reduces the chances of rear wheel lockup during normal braking