For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Were you sent here from the Radio/Audio System Check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Check the tape player for an obstruction through the tape door. Does an obstruction exist? | -- | Go to Step 3 | Go to Step 4
3 |

1. Remove the obstruction. Care should be taken to avoid damaging the tape player.
2. Inspect and clean the tape head and all moving parts.
3. Use the cleaning cassette.
4. Use the diagnostic tape from the J 39916-A .

Does the test tape operate properly?

--

Go to Radio/Audio System Check

Go to Step 4

4 | Replace the radio. Refer to Radio Replacement . Is the replacement complete? | -- | Go to Radio/Audio System Check | --
5 | The fault is with the cassette tape. Replace the faulty cassette. Is the replacement complete? | -- | Go to Radio/Audio System Check | --