For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the turn signal headlamp switch to the HEAD position. |

• | The low beam headlamps are ON.

• | The high beam headlamps are OFF.

• | Headlamps Inoperative - Low Beams

• | Headlamps Inoperative - Left Low Beam

• | Headlamps Inoperative - Right Low Beam

2 | Pull the turn signal/ headlamp switch back to the PASS position. |

• | The high beam headlamps are ON while the switch is held.

• | The high beam indicator is ON.

Headlamps Inoperative - High Beams

3 | Push the turn signal/ headlamp switch forward to the HIGH position. | The high beam headlamps are ON. |

• | Headlamps Inoperative - High Beams

• | Headlamps Inoperative - Left High Beam

• | Headlamps Inoperative - Right High Beam

• | Low and High Beams Headlamps Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.