For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column-Standard Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column - Standard
2 | Verify the ignition lock cylinder exhibits high lock effort. Does the ignition lock cylinder exhibit high lock effort? | Go to Step 3 | System OK
3 | Inspect the lock cylinder case for damage. Is the lock cylinder case damaged? | Go to Step 6 | Go to Step 4
4 | Inspect the lock cylinder for damage. Is the lock cylinder damaged? | Go to Step 7 | Go to Step 5
5 | Inspect the ignition switch for damage. Is the ignition switch damaged? | Go to Step 8 | Go to Step 3
6 | Replace the lock cylinder case. Refer to Ignition Lock Cylinder Case Replacement - On Vehicle . Did you complete the repair? | Go to Step 9 | --
7 | Replace the lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle . Did you complete the repair? | Go to Step 9 | --
8 | Replace the ignition switch. Refer to Ignition Switch Replacement - On Vehicle . Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3