For 1990-2009 cars

1. Remove the key from the ignition switch.
2. Install the yellow 2-way connectors to the driver and passenger seat modules (1).
3. Connect the connectors and lock the connectors with the connector lock levers.
4. Install the yellow 2-way connector to the inflatable restraint IP module pigtail (1).

Connect the connector and lock the connector with the connector lock lever.

5. Install the IP compartment (2). Refer to Instrument Panel Compartment Replacement .
6. Install the yellow 2-way connector (1) for the inflatable restraint steering wheel module coil.

Connect the connector and lock the connector with the connector lock lever.

7. Install the lower steering column trim cover.
8. Install the CIG and IGN Fuses to the junction block (1).
9. Staying well away from both air bags, turn the ignition switch to the ON position. Verify that the AIR BAG warning lamp comes on for approximately 6 seconds and then stays OFF. If the AIR BAG warning lamp does not operate as described, refer to SIR Diagnostic System Check .