For 1990-2009 cars

1. Remove the intermediate brake hub (2) and the intermediate one-way clutch from the intermediate brake (1).
2. Inspect the intermediate brake piston operation by applying 392-785 kPa (57-114 psi) of compressed air into the intermediate brake apply passage (1). Ensure that the intermediate brake piston applies and releases smoothly.
3. Remove the intermediate brake drum snap ring (1) from the transaxle case.
4. Remove the intermediate brake drum (1) and the piston from the transaxle case (2).
5. Remove the intermediate brake piston return spring (1) from the transaxle case (2).
6. Remove the following components (1) from the transaxle case (2):

• | The 3 intermediate brake discs

• | The 3 intermediate brake plates

• | The intermediate brake flange