For 1990-2009 cars

# Information on 2000 bill 101 French Label Installation Procedure

Subject: | Information on 2000 Bill 101 French Label Installation Instructions

Models: | 2000 Passenger Cars and Trucks

| 2001 Oldsmobile Aurora

Attention: | This bulletin is applicable to GM of Canada dealers/retailers only.

### Format

This bulletin contains information on the 2000 Bill 101 French Label Installation Instructions. The following format is used:

#### Section I -- Passenger Car Label Information

• | General

• | Engine Compartment

• | Interior Compartment

• | Luggage Compartment

#### Section II -- Light Duty Truck Label Information

• | General

• | Engine Compartment

• | Interior Compartment

• | Vehicle Exterior

#### Section III -- Medium Duty Truck Label Information

• | General

• | Engine Compartment

• | Interior Compartment

• | Vehicle Exterior

Important: Sections I and II are referenced on 2000 Passenger Car drawing 52369730 Sheets 2 and 3 and Light Duty Truck Chart drawing 52369757 Sheets 2 and 3. Section III referenced on Medium Duty Truck drawing 52369780.

### Section I -- Passenger Car Label Information

General -- All 2000 Passenger Cars and 2001 Oldsmobile Aurora

Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Locate labels next to corresponding English labels, unless otherwise noted. Both labels must be readable.

Engine Compartment

1. A/C Label (R-134a)

Place labels adjacent to the English labels if space permits and, if not, they are to be placed in a prominent position so that viewers will be aware the vehicle uses R-134a refrigerant.

• | C, H, G, E, K-Car use 52367054 -- A/C Refrigerant Charge

• | W-Car use 52367382 -- A/C Refrigerant Charge

• | J, N-Car and U-Van use 52366392 -- A/C Refrigerant Charging

• | U-Van and Saturn use 52366391 -- A/C R-134a Refrigerant Usage and Charge Caution

• | Catera use 52368309 -- A/C Caution and Charge Information

• | C, H, G-Car part of combined label 52366710

• | F-Car part of combined label 52369842

• | Y-Car part of combined label 52369841

• | Saturn part of combined label 52367175

2. Accessory Belt Routing Label

Place label adjacent to engine label

• | Catera use 52368046 for U.S. No. 95529598

• | Saab use 52366363 for U.S. No. 4359444

• | W-Car with 3800 V6 use 52369850 for U.S. No. 24504969

• | W-Car with 3800 Supercharged V6 use 52369851 for U.S. No. 24507218

• | W-Car with 3400 V6 use 52369853 for U.S. No. 24507820

3. Battery Caution Labels

Battery labels are placed on top of the existing label.

• | Use 52368737 for Delco Batteries with a Service Tab on the RH side of the battery

• | Use 52368738 for Delco Batteries with a Service Tab on the LH side of the battery (The cutout should allow the tab to be lifted)

4. Combined Labels

Place adjacent to English label

• | C, H, G-Car use 52366710 -- A/C Refrigerant, Fan Caution, Fluid Usage and SIR Notice

• | E, K-Car use 52367711 -- Engine Cooling and Inflatable Restraint System Notice

• | F-Car use 52369842 -- Fan Blade, Inflatable Restraint, Engine Cooling, A/C Refrigerant Notice

• | Y-Car use 52369841 -- A/C, Special Engine Oil, Inflatable Restraint and Engine Cooling

• | Saturn use 52367175 -- Fan Caution and A/C

5. DEX-COOL® Notice Label

• | C, H, G, J, N-Car, Saturn and Catera use 52368325, place adjacent to English label

• | W-Car use 52368212, place adjacent to English label

• | U-Van use 52368213, place adjacent to English label

6. Engine Jump Start Notice Label

Place adjacent to English label, passenger shock tower

E, K-Car use 52369430

7. Engine Oil Fill Label

Place label on Fan shroud or Radiator support assembly

C, H, G, F, E, K, J, N, W-Car, U-Van and Saturn use 52367565

8. Fan Caution Label

If vehicle is equipped with an English label, place a bilingual label over it. Otherwise, place the French label adjacent to the English embossed message on fan shroud.

• | J, N, W, Y-Car, Catera and U-Van use label 52355271

• | Saab use 52366361

• | C, H, G-Car part of combined label 52366710

• | F-Car part of combined label 52369842

• | Saturn part of combined label 52367175 (Fan Caution and A/C)

9. Fuel Flammable Caution Label

Wrap four (4) labels around fuel line adjacent to English label

• | If no English labels present, there is no need to use the French

• | All vehicles use 52362963

10. Fuse Block Identification Label

Place adjacent to fuse block cover or on fuse block cover (as required)

Do not cover fuse location diagram

• | C, H, G, E, K, J, N, W, F, Y, M-Car and U-Van use 52367387

• | Catera use 52368327

11. Hood Prop Rod Label

Place label adjacent to slot in hood inner panel

J, N, M-Car, U-Van and Saturn use 52354520

12. SIR Caution Label

Place label under hood on radiator support assembly or adjacent to English label (with SIR system)

• | J, M-Car and Saturn use 52363000

• | C, H, G-Car part of combined label 52366710

• | Y-Car part of combined label 52369841

• | E, K-Car part of combined label 52367711

13. Vehicle Lifting Notice Label

Place on radiator support assembly or air intake duct

J, N-Car use 52369423

14. Windshield Wiper System Caution Label

Place label adjacent to the existing English

U-Van use 52367176

Interior Compartment

1. Child Security Lock Information Label (Rear Door Window)

Place adjacent to English label on inside rear door glass

C, H, G, E, K, J, N, W, M-Car, Saturn, Saab and U-Van use 52365626

2. Child Security Lock Operation Instruction Label (near Lock Lever)

Place adjacent to English label near lock lever

• | J-Car use 52362462

• | Saturn use 52367466 (LH) and 52367467 (RH)

• | C, H, G, E, K, N, W-Car use 52368211 (LH) and 52368210 (RH)

• | Catera use 52368047 (LH) and 52368048 (RH)

• | M-Car use 52363755

• | U-Van use 52366354 (rear side door, sliding)

3. Convenience Net Information Label

Place adjacent to English label

U-Van use 52365608

4. Convertible Top Operation Instruction Card

Place in stowage console

Y-Car use 52369262

5. Do Not Overheat Unit Label

Place adjacent to English label

U-Van use 52369520

6. Folding Top Damage Label

Place adjacent to English label

F-Car (convertible) use 52366042

7. Fuse Block Identification Labels

Place adjacent to fuse block cover or on fuse block cover (as required)

Do not cover fuse location diagram

• | C, H, G, E, K, J, N, W, F, Y, M-Car and U-Van use 52367387

• | Catera use 52368327

8. Inflatable Restraint Instrument Panel Module Tag

Fasten to English tag on instrument panel (all except Y-Car)

On Y-Car fasten to Grab bar on instrument panel

C, H, G, E, K, J, N, W, F, Y-Car, Catera, Saturn and U-Van use 52368736

9. Inflatable Restraint System Caution Alert Label

Place on sun-visor adjacent to English label when required

J-Car use 52368732

10. Jack Assembly Caution Label

Place adjacent to English label (on jack)

U-Van use 52367590

11. Jack Usage Label

Place adjacent to English label

U-Van use 52367977

12. Outside Rear View Mirror Warning (French) Label

Place on RH front door interior glass, in-line with outside rear view mirror

All Models -- C, H, G, E, K, J, N, W, F, Y, M-Car, Catera, Saturn, Saab and U-Van use 52369536

13. Passenger Front Seat Belt SIR Information Caution Label

Place on passenger front door lock pillar above striker

• | C, H, G, E, K, J, N, W, F, Y, M-Car and Saturn use 52369796

• | U-Van use 52367461

14. Power Sliding Door Warning Label

Place adjacent to English label

U-Van use 52367976

15. Rear Seat Location Information Labels

Place adjacent to English labels (15 labels showing seat locations)

U-Van use 52367973

16. Rear Seat Operation Instructions (ENG/FR) Label

Place adjacent to English labels

U-Van use 52368190, 52368191, 52368192, 52368193 and 52368194

17. Rear Seat Outer Belt Retainer Instructions Label

Place on rear door lock pillar above striker

• | C, H, G, W-Car and Catera use 52369794

• | U-Van use 52369844

18. Roof Special Care Notice Label

Place adjacent to English label

Y-Car 52367640

19. Battery Caution Labels

Place label on battery under rear seat

C, H, G, E, K-Car use 52369839 (under rear seat)

20. Battery Sulfuric Acid Fume Caution Labels

Place label around battery cable under rear seat

C, H, G, E, K-Car use 52366746 (under rear seat)

21. Theft Deterrent System Label

Place adjacent to English label on front door glass

• | Catera use 52368216

• | Saturn use 52368217

• | Saturn Security System Card 52368734, place in glove box of Saturn vehicle

Luggage Compartment

1. Jack Assembly Caution Label

Place adjacent to English label (on jack)

• | C, H, E, K, J, N, W-Car and Saturn use 52367590

• | M-Car use 52362566

2. Jack Usage Label

Place in rear compartment stowage area with English instructions

• | C-Car use 52361492

• | G, H-Car use 52369799

• | G-Car use 52366743

• | J, N-Car use 52364449

• | F-Car use 52366905

• | W-Car (Grand Prix/Century/Regal/Intrigue) use 52368730

• | W-Car (Lumina) use 52366252

• | W-Car (Monte Carlo) use 52369849

• | W-Car (Impala) use 52369848

• | E, K-Car use 52368203

• | M-Car use 52362563

• | Saturn "S" Series (Z-Car) use 52365012

• | Saturn "L" Series (J-Car) use 52369854

• | Saab use 52366358

• | Catera use 52368310

### Section II -- Light Duty Truck Label Information

General -- C/K, S/T-Truck and G, L/M-Vans, Tracker, Trooper, Rodeo, Hombre

Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Locate labels next to corresponding English labels, unless otherwise noted. Both labels must be readable.

Engine Compartment

1. A/C R-134a Refrigerant Usage and Charge Caution Label

Place on radiator support assembly

For all R-134a vehicles use 52366391

2. A/C Refrigerant Charging R-134a Label

Place on radiator support assembly

For all R-134a vehicles use 52366392

3. Battery Caution Labels

Battery labels are placed on top of the existing label.

• | Use 52368737 for Delco Batteries with a Service Tab on the RH side of the battery

• | Use 52368738 for Delco Batteries with a Service Tab on the LH side of the battery (The cutout should allow the tab to be lifted)

4. Battery Charge Indicator Label

Place on battery

Tracker use 52362523

5. DEX-COOL® Label

Place on radiator support

C/K, S/T-Truck, G, L/M-Van and Hombre use 52368326

6. Engine Coolant and Inflatable Restraint System Notice (Diesel)

• | C/K-Truck (Z71 Utility, 200 greater than 8500 GVWR, 300 & Cad. Escalade/GMC Denali), S/T-Truck, G, L/M-Van and Hombre use 52369591

• | C/K-Truck (Sierra/Silverado) use 52369836

7. Accessory Belt Routing Label

Place adjacent to English label

C/K-Truck (Sierra/Silverado) use 52369831

8. Engine Oil Fill Label (ENG/FR)

Place on radiator support assembly

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52367565

9. Fan Blade Caution Label (ENG/FR)

Place on fan shroud assembly

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52362522

10. Fuel Flammable Caution Label

Wrap four (4) labels around fuel line adjacent to English label

If no English labels present, there is no need to use the French

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52362963

11. Fuse Block Identification Labels

Place adjacent to fuse block cover or on fuse block cover (as required)

Do not cover fuse location diagram

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52367387

12. High Voltage Lamp Label

Place adjacent to English label, on lamps or near lamps

S/T-Truck use 52369581

13. Hood Prop Rod Label (ENG/FR)

Place adjacent to slot in hood inner panel

S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52354520

14. Inflatable Restraint System Label

Place on radiator support assembly

All models (except Tracker) -- C/K, S/T-Truck, G, L/M-Van, Trooper, Rodeo and Hombre use 52367053

15. Radiator Cap Label (ENG/FR)

Place on radiator cap

Tracker use 52356339

16. Front Torsion Bar Adjustment Caution Label

Place adjacent to engine label on torsion bar support assembly

C/K-Truck (Sierra/Silverado) use 52369834

Interior Compartment

1. A/C Filter Information Label

Place adjacent to English label

C/K-Truck (Sierra/Silverado) use 52369424

2. Child Security Lock Information Label

Place adjacent to English label on inside rear door glass

C/K (Z71 Utility, 200 greater than 8500 GVWR, 300 & Cad. Escalade/GMC Denali), S/T-Truck, G, L/M-Van, Tracker, Trooper and Rodeo use 52365626

3. Child Security Lock Operation Instruction

Place adjacent to English label unless otherwise noted

• | C/K and S/T-Truck use 52367466 (LH) and 52367467 (RH), place adjacent to English label on inner rear door panel

• | G-Van use 52362462, place adjacent to English label on rear cargo door

• | G-Van use 52366354, place adjacent to English label on rear side sliding door

• | G-Van use 52368210, place adjacent to English label on rear side swing-out door

• | L/M-Van use 52366354, place adjacent to English label on rear side sliding door

• | Tracker, Rodeo use 52362462, place on rear door panel near lock lever

• | Trooper use 52363755, place on rear door panel near lock lever

4. Convenience Net Information Label

Place adjacent to English label

Tracker use 52365608

5. Engine Start Procedure Notice Label (Diesel)

Place adjacent to English label

C/K-Truck and G-Van use 52367143

6. Fuse Block Identification Labels

Place adjacent to fuse block cover or on fuse block cover (as required)

Do not cover fuse location diagram

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52367387

7. Humidity Removal Tag

Place on back of existing English tag

Tracker use 52366346

8. Inflatable Restraint Instrument Panel Module Tag

Fasten to English tag on instrument panel

• | C/K-Truck, G, L/M-Van, Tracker, Trooper and Rodeo use 52368736

• | S/T-Truck and Hombre use 52368735 and 52368736

9. Inflatable Restraint System Caution (Alert) Label

Place adjacent to English label on sun-visor

Please note sun-visor labels are often of very strong adhesive, care should be taken that they are applied properly as adjustment may prove impossible. Should space not be available and the headlining used, please be sure that the sun-visor in the up position covers the label.

S/T-Truck, G-Van and Hombre use 52368732

10. Interior Side Door Operation Instruction Notice Label

Place adjacent to English label

G-Van use 52367713

11. Jack Assembly Caution Label

Place adjacent to English label (on jack)

• | C/K, S/T-Truck, G, L/M-Van and Hombre use 52367590

• | C/K (157-15900) and (257-25900) use 52369837

• | Tracker use 52362520

12. Jack Assembly Caution and Usage Tag

Place adjacent to English label

• | C/K-Truck (Sierra/Silverado)

• | C/K (Pickup and Extended Cab) use 52369429

• | C/K (Utility and Suburban) use 52369847

• | C/K-Truck (Z71 Utility, 200 greater than 8500 GVWR, 300 & Cad. Escalade/GMC Denali)

• | C/K (310,314-03) use 52366250

• | C/K (100-20006-16) use 52366249

• | C/K (Crew Cab) use 52366253

• | C/K (Pickup except Crew Cab) use 52366254

• | S/T-Truck use 52367171

• | Utility use 52367211

• | Pickup, Extended Cab use 52367210

• | G-Van use 52368195

• | Hombre use 52367210

• | Tracker use 52362519

13. Outside Rear View Mirror Warning (French) Label

Place on RH front door interior glass, in-line with outside rear view mirror

All models -- C/K, S/T-Truck, G, L/M-Van, Tracker, Trooper, Rodeo and Hombre use 52369536

14. Passenger Front Seat Belt SIR Information Caution Label

Place on passenger front door lock pillar above striker

C/K, S/T-Truck, G-Van, Tracker, Hombre, Trooper and Rodeo use 52369795

15. Rear Seat Outer Belt Retainer Instructions Label

Place on rear door lock pillar above striker

C/K-Truck (Sierra/Silverado), S/T-Truck use 52369844

16. Rear Door Operating Instructions Notice Label

Place adjacent to English label

C/K-Truck (Z71 Utility, 200 greater than 8500 GVWR, 300 & Cad. Escalade/GMC Denali) use 52369855

17. Rear Seat Latch Caution Label

Place adjacent to English label on rear seat assembly

C/K-Truck (Sierra/Silverado) use 52369835

18. Rear Seat Belt and Seat Latch Caution Label

Place adjacent to English label

G-Van use 52367972

19. Rear Seat Lock Pin Storage Instructions Label

Place adjacent to English label

G-Van use 52368214

20. Side Access Panel Notice Label

Place adjacent to English label

C/K, S/T-Truck and Hombre use 52367460

21. Utility Vehicle Handling Label

Place adjacent to English label

S/T-Truck, Tracker, Hombre, Trooper, Rodeo use 52354648

22. Window Fog Electro-Static Label

Place adjacent to English label on Instrument Panel

Trooper and Rodeo use 52369434

23. Active Transfer Case Caution Label

Place adjacent to English label

C/K-Truck (Sierra/Silverado), S/T-Truck use 52369830

Vehicle Exterior

1. Spare Tire Cover Installation Label

Place adjacent to English label inside cover

Trooper use 52369431

2. Fuel Recommendation Label

Place on fuel filler door

S-Truck (4 cylinder) use 52369838

3. Do Not Tow Notice Label

Place adjacent to English label on rear bumper

S/T-Truck use 52369840

### Section III -- Medium Duty Truck Label Information

General -- MD Truck (2000) (C6-7, F6-7)

Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface.

Locate labels next to corresponding English labels, unless otherwise noted. Both labels must be readable.

Engine Compartment

1. A/C R-134a Labels

Place adjacent to existing English label

• | C6-7 use 52366391 (Refrigerant Usage and Charge Caution)

• | C6-7 use 52366392 (A/C Refrigerant Charging R-134a)

2. Air Conditioning Label

Place adjacent to existing English label

F6-7 use 52367985

3. Battery Label

Place bilingual battery labels over existing labels as indicated:

• | C6-7 use 52363359 over 1981733

• | C6-7 use 52363360 over 1981734

• | C6-7 use 52363361 over 1981730

• | C6-7 use 52363362 over 1981735

• | C6-7 use 52363367 over 1981736

4. Battery Tray Removal Label

Place adjacent to English label

C6-7 use 52366748

5. Caution Moving Parts Label

Place adjacent to English label

F6-7 use 52367982

6. Clutch Caution Tag (on Bell Housing)

Place adjacent to English label on Bell Housing

C6-7 and F6-7 use 52367980

7. Electric Box Connector Notice Label

Place adjacent to existing English label

F6-7 use 52367981

8. Ether Notice Label

Place adjacent to existing English label

• | C6-7 use 52367461 and 52368199

• | F6-7 use 52368199

9. Ether Start Notice Label

Place label on air cleaner

C6-7 use 52363056

10. Fuel Miser Label

Place adjacent to existing English label

C6-7 use 52367383

11. Radiator Fill Notice (Diesel Caterpillar Coolant Label)

Place adjacent to existing English label

C6-7 use 52367391

12. Synthetic Lube Label

Place adjacent to existing English label

F6-7 use 52367979

13. Wiper Can Cycle Label

Place adjacent to existing English label

F6-7 use 52369783

Interior Compartment

1. 2-Speed Rear Axle Shift Label

Place on headliner

C6-7 use 52363112

2. Daytime Running Lights Label

Place on instrument panel

C6-7 use 52362143

3. Diesel Start Fluid Warning Label

Place adjacent to English label on sun-visor

C6-7 use 52363052

4. Engine Start Procedure Notice (Diesel) Label

Place on sun-visor (fuel unique to Canada)

C6-7 use 52367143

5. Rear Axle Operations Label

Place on headliner

C6-7 use 52363054

6. Transmission Shift Instruction Labels

Place on headliner

• | C6-7 use 52363057, adjacent to 2018123

• | F6-7 use 52367978, adjacent to 15739200

Vehicle Exterior

1. Avoid Drilling Label

Place on frame rail adjacent to English label

C6-7 use 52362153

2. Caution Tilt Cab Labels

F6-7 use 52367974 adjacent to English label

F6-7 use 52367975 over existing English label on rear of cab -- LH side

3. No Step Label

Place adjacent to English label

F6-7 use 52367984