For 1990-2009 cars

### Removal Procedure

1. Straighten the left wiper tabs (2) until the windshield wiper element can slide freely.
2. Slide the wiper element (3) out through the windshield wiper blade (1).

### Installation Procedure

1. Slide the windshield wiper element (3) completely through the windshield wiper blade (1).
2. Bend down the wiper tabs (2) to secure the wiper element in position.