For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Checks the door power LOCK function of the RKE transmitters.
1 | Test the power door lock function by pressing the door mounted LOCK/UNLOCK switch to the LOCK position. Does the power door LOCK function operate properly? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 |

1. Make sure that the ignition key is removed from the ignition.
2. Press the power door LOCK button on the transmitter once.

Do all of the doors lock?

--

Go to Remote Keyless Entry System Check

Go to Step 3

3 | Test the door lock function with a known good transmitter. Do all the doors lock? | -- | Go to Step 4 | Go to Step 5
4 | Replace the RKE transmitter. Refer to Transmitter Replacement in Keyless Entry. Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --
5 |

1. Disconnect the remote control door lock receiver connector. Refer to Remote Control Door Lock Receiver Replacement in Keyless Entry for access.
2. Connect a J 36169-A between terminal 15 of the remote control door lock receiver connector and a known good ground.

Do all the doors lock?

--

Go to Step 7

Go to Step 6

6 | Repair the open between terminal 15 of the remote control door lock receiver connector and SP252 . Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --
7 | Replace the remote control door lock receiver. Refer to Remote Control Door Lock Receiver Replacement in Keyless Entry. Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --