For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column
2 | Verify that the steering column tilt function is inoperative. Is the steering column tilt function inoperative? | Go to Step 3 | System OK
3 | Inspect the steering column wiring harness for proper routing. Is the harness routing proper? | Go to Step 5 | Go to Step 4
4 | Reroute the steering column wiring harness. Did you complete the adjustment? | Go to Step 6 | --
5 | Replace the steering column. Refer to Steering Column Replacement . Did you complete the repair? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3