For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the ON position.
2. Leave the windshield wiper/washer switch in the OFF position.
3. Pull the windshield wiper/washer switch for 2 to 4 seconds and release.

• | Wipers operate at low speed.

• | Washer sprays windshield as long as washer switch is held in the ON position.

• | After releasing switch, washer stops and wipers return to park position after 1 to 4 sweeps.

• | Washers Inoperative

• | Wipers All Modes and Washer Inoperative

• | Washers Always On

2 | Move the windshield wiper/washer switch to the LO position. | Wipers run continuously at low speed. |

• | Wipers Low Mode Inoperative, High Mode Operates

• | Wipers All Modes Inoperative

3 | Move the windshield wiper/washer switch to the HI position. | Wipers run continuously at high speed. |

• | Wipers All Modes Inoperative

• | Wipers High Mode Inoperative, Low Mode Operates

4 | Move the windshield wiper/washer switch to the OFF position. | Wipers return to the park position at low speed. |

• | Wipers Always On

• | Wipers Blades Do Not Park

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.