For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Drill out the 3 front door speaker rivets.
3. Disconnect the speaker electrical connector.
4. Remove the front door speaker from the vehicle.

### Installation Procedure

1. Connect the speaker electrical connector.
2. Install the speaker (1) to the door. Secure the speaker with 3 rivets (2).
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.