For 1990-2009 cars

#### Tools Required

• | J 36850 Transjel® Transmission Assembly Lubricant

• | J 23327-1 Clutch Spring Compressor

• | J 35683 First and Reverse Brake Piston Compressor

1. Apply J 36850 to the new 1st-reverse brake piston seals (2) .
2. Install the 1st-reverse brake piston (1) into the transaxle case with the cup facing upward.
3. Install the 1st-reverse brake piston return spring (2) into the transaxle case.
4. Install the J 23327-1 with a J 35683 and compress the 1st-reverse brake piston return spring until you can install the 1st-reverse brake piston return spring snap ring (1).
5. Install the 1st-reverse brake piston return spring snap ring into the transaxle case.
6. Remove the J 23327-1 and theJ 35683 from the transaxle case.