For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 | Are the Power Locks working properly? | -- | Go to Step 4 | Go to Step 3
3 | Repair the open in the WHT/BLK wire between SP551 to G200 or replace the SP551. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
4 |

1. Turn the ignition switch to the RUN position.
2. Disconnect the LH window/door lock switch connector.
3. Using a test lamp, probe the connector cavity 10 to ground.

Does the test lamp illuminate?

--

Go to Step 5

Go to Step 6

5 | Replace the LH window/door lock switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
6 | Repair the open in the BLK wire and/or replace the SP551, SP252, and/or junction block 1, as needed. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --