For 1990-2009 cars

### Removal Procedure

1. Remove the screw (3) from each side of the front floor rear console (2) which secures the rear console to the front floor front console (1).
2. Remove the 2 bolts (1) from the rear compartment of the rear console (2).
3. Raise the parking brake lever.
4. Remove the front floor rear console (1) from the vehicle.

### Installation Procedure

1. Install the front floor rear console (1) to the vehicle.
2. Lower the parking brake lever

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the 2 bolts (1) to the rear compartment of the rear console.

Tighten
Tighten the front floor rear console bolts to 15 N·m (11 lb in).

4. Install the screw (3) to each side of the front floor rear console (2) which secures the rear console to the front floor front console (1).