For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Pull the plastic locking tab on the rear compartment courtesy lamp protection shield (3).
3. Open the lamp protection shield (3).
4. Remove the rear compartment courtesy lamp bulb (2) from the lamp socket (1).

### Installation Procedure

1. Install the rear compartment courtesy lamp bulb (2) to the lamp socket (1).
2. Close the rear compartment courtesy lamp protection shield (3).
3. Close the rear compartment lid.