For 1990-2009 cars

1. Remove the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.
2. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
3. Remove the instrument panel (IP) compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
4. Remove the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
5. Remove the radio. Refer to Radio Replacement in Entertainment.
6. Remove the temperature control cable from the clip at the HVAC module assembly.
7. Set the temperature dial to the coldest position.
8. Hold the door lever fully forward.
9. Install the cable to the clip.
10. Test the cable for smooth operation.
11. Test that the door opens fully in both directions.
12. Install the radio. Refer to Radio Replacement in Entertainment.
13. Install the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
14. Install the IP compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
15. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
16. Install the center console trim bezel. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.