For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition key to LOCK.
2. Remove the ignition key.
3. Exit the vehicle and close all doors.
4. Press the transmitter LOCK button for approximately 1 second and release.

• | All doors lock.

• | The parking lamps and tail lamps flash once to confirm operation.

• | Keyless Entry System Inoperative

• | Door Lock Inoperative Using Transmitter - Left Side Front

• | Door Lock Inoperative with Transmitter - All

2 | Press the transmitter UNLOCK button once for approximately 1 second and then release. |

• | The left front door unlocks.

• | The parking lamps and tail lamps flash twice to confirm operation.

• | The dome light illuminates for approximately 15 seconds and then turns off.

• | The left front door locks after approximately 30 seconds.

• | Door Unlock Inoperative with Transmitter - Left Side Front

• | Door Lock Inoperative Using Transmitter - Left Side Front

3 | Press the transmitter UNLOCK button twice within 5 seconds. |

• | All of the doors unlock.

• | The parking lamps and tail lamps flash twice to confirm operation.

• | The dome light illuminates for approximately 15 seconds and then turns off.

• | All of the doors lock after approximately 30 seconds.

• | Door Unlock Inoperative with Transmitter - All

• | Door Lock Inoperative with Transmitter - All

4 |

1. Press the transmitter UNLOCK button twice within 5 seconds.
2. Open and close any of the vehicle doors within approximately 30 seconds.

• | All of the doors unlock.

• | The parking lamps and tail lamps flash twice to confirm operation.

• | The dome light illuminates for approximately 15 seconds and then turns off.

• | All of the doors remain unlocked after approximately 30 seconds.

Door Unlock Inoperative with Transmitter - All

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.