For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the following components from the vehicle:

• | The 4 rear compartment trim panel plastic retainers (2)

• | The rear compartment trim panel (1)

3. Remove the tail lamp socket (3) from the tail lamp.
4. Remove the tail lamp bulb from the lamp socket (3).

### Installation Procedure

1. Install the tail lamp bulb to the lamp socket (3).
2. Install the tail lamp socket (3) to the tail lamp.
3. Install the rear compartment trim panel (1) to the vehicle. Secure the trim panel with the 4 plastic retainers (2).
4. Close the rear compartment lid.