For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Starting System Check? | Go to Step 2 | Go to the Starting System Check
2 |

1. Test for battery voltage at the starter solenoid terminal S.
2. Engage the parking brake and place the gear shift lever in N or the manual selector lever in P or N.
3. Depress the clutch pedal fully (manual transaxle).
4. Turn the ignition switch to the START position.

Is battery voltage present?

Go to Step 3

Go to Step 5

3 | Test for an open in the BLK/RED wire between the battery and the starter solenoid. Is an open present? | Go to Step 21 | Go to Step 4
4 | Replace the starter solenoid. Refer to Starter Motor Replacement and Starter Motor Overhaul . Is the repair complete? | Go to the Starting System Check | --
5 | Test for an open in the BLK wire between the starter relay terminal 2 and the starter solenoid terminal S. Refer to

#### Fuse and Relay Block 1

(1) | ST Relay
(2) | HEAD Relay
(3) | EFI or F-HTR Relay
(4) | Fuse Puller
(5) | ENGINE MAIN Relay
(6) | HORN Relay
(7) | AM1 Fuse 50A
(8) | RDI Fuse 30A
(9) | FAN Relay
(10) | ALT-S Fuse 7.5A
(11) | Empty
(12) | Not Used
(13) | HORN Fuse 20A
(14) | Not Used
(15) | Not Used
(16) | AM2 Fuse 30A
(17) | HAZARD Fuse 20A
(18) | DOME Fuse 20A
(19) | ALT Fuse 100A
(20) | ABS Fuse 50A
(21) | MAIN Fuse 50A
(22) | Not Used
(23) | Fuse and Relay Block 1

in Wiring Systems.

Is an open present?

Go to Step 21

Go to Step 6

6 | Test for voltage at the starter relay terminal 1. Is battery voltage present? | Go to Step 9 | Go to Step 7
7 | Test for an open between the starter relay terminal 1 and the MAIN fuse in fuse and relay block 1. Is an open present? | Go to Step 18 | Go to Step 8
8 | Repair the open between the battery positive terminal and the MAIN fuse in fuse and relay block 1. Replace fuse and relay block 1 if necessary. Refer to Underhood Fuse Block Replacement . Is the repair complete? | Go to the Starting System Check | --
9 | Test for an open in the WHT/BLK wire between the starter relay terminal 4 and G103. Is an open present? | Go to Step 21 | Go to Step 10
10 | Test for battery voltage at the starter relay terminal 3 with the ignition switch in the START position. Is battery voltage present? | Go to Step 23 | Go to Step 11
11 |

1. Inspect that the AM2 fuse is not open.
2. Test for battery voltage at the ST fuse in junction block 2 with the ignition switch in the START position.

Is battery voltage present?

Go to Step 15

Go to Step 12

12 |

1. Test for an open between the AM2 fuse and connector 3 terminal 8 in fuse and relay block 1.
2. Test for an open between the ST relay terminal 3 and connector 8 terminal 3 in fuse and relay block 1. Refer to

   #### Junction Block 2

   (1) | Not Used
   (2) | ST Fuse 5A
   (3) | D/L Fuse 30A
   (4) | Fog Fuse 15A
   (5) | S-HTR Fuse 15A
   (6) | Not Used
   (7) | CIG Fuse 15A
   (8) | DEF Fuse 40A
   (9) | Dome Noise Filter
   (10) | POWER Fuse 30A
   (11) | Short Pin
   (12) | C2
   (13) | C5
   (14) | C4
   (15) | ECU-B Fuse 7.5A
   (16) | C3
   (17) | C1
   (18) | Not Used
   (19) | DEF-I/UP Fuse 10A
   (20) | WIP Fuse 20A
   (21) | GAUGE Fuse 10A
   (22) | Not Used
   (23) | TURN Fuse 7.5A
   (24) | STOP Fuse 15A
   (25) | IGN Fuse 7.5A
   (26) | TAIL Fuse 15A
   (27) | ECU-IG Fuse 10A
   (28) | OBD Fuse 7.5A
   (29) | Not Used

   in Wiring Systems.

Is an open present?

Go to Step 18

Go to Step 13

13 | Test for an open in the BLK/RED wire between the ignition switch fuse and relay block 1 (including junction block 2). Is an open present? | Go to Step 21 | Go to Step 14
14 | Test for an open in the RED wire between the ST fuse in junction block 2 and the ignition switch. Is an open present? | Go to Step 21 | Go to Step 22
15 |

• | Test for an open in the BLK /WHT wire between the PNP switch (automatic transaxle) and the ST fuse.

• | Test for an open in the BLK /WHT wire between the CPP switch (manual transaxle) and the ST fuse.

Is an open present?

Go to Step 21

Go to Step 16

16 |

• | Test the PNP switch for continuity in the park and neutral positions (automatic transaxle).

• | Test the CPP switch for continuity with the clutch pedal depressed (manual transaxle).

Did the switch test OK?

Go to Step 17

Go to Step 20

17 |

1. Test for an open in the BLK wire between the PNP switch (automatic transaxle) and connector 8 terminal 3 of fuse and relay block 1.
2. Test for an open in the BLK wire between the CPP switch (manual transaxle) and connector 8 terminal 3 of fuse and relay block 1.

Is an open present?

Go to Step 21

Go to Step 18

18 | Replace fuse and relay block 1. Refer to Underhood Fuse Block Replacement . Is the repair complete? | Go to the Starting System Check | --
20 |

1. Replace the PNP switch (automatic transaxle). Refer to Park/Neutral Position Switch in Automatic Transmission-4 Speed-MS7.
2. Replace the CPP switch (manual transaxle). Refer to Clutch Pedal Position Switch Replacement in Clutch.

Is the repair complete?

Go to the Starting System Check

--

21 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to the Starting System Check | --
22 | Replace the ignition switch. Refer to Ignition Switch Replacement - On Vehicle in Steering Wheel and Column-Std or Ignition Switch Replacement - On Vehicle in Steering Wheel and Column-Tilt. Is the repair complete? | Go to the Starting System Check | --
23 | Replace the starter relay. Is the repair complete? | Go to the Starting System Check | --