For 1990-2009 cars

## Window Guide Channel Replacement - Front Door Rear

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement .
2. Pull the window run channel (1) loose along the rear window guide (2).
3. Remove the following components from the door:

• | The bolt (1)

• | The rear window guide

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear window guide to the door. Secure the guide with the bolt (1).

Tighten
Tighten the rear window guide bolt to 8 N·m (71 lb in).

2. Press the window run channel (1) into the rear window guide (2).
3. Install the front door window. Refer to Front Side Door Window Replacement .