For 1990-2009 cars

## Rear Seat Back Cushion Frame Replacement AM9

### Removal Procedure

1. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
2. Remove the rear seat back cushion. Refer to Rear Split Folding Seat Back Replacement .
3. Remove the rear seat shoulder belt guide from the rear seat back cushion by gently prying loose.
4. Remove the plastic retainers which secure the seat back cushion cover (1) to the back of the seat.
5. Cut and remove the hog rings around the perimeter of the back of the rear seat back cushion (1).
6. Remove the rear seat back cushion cover from the cushion.
7. Remove the rear seat back cushion pad from the frame.

### Installation Procedure

1. Install the rear seat back cushion pad to the frame.
2. Install the rear seat back cushion cover to the seat back frame.
3. Use hog ring pliers (1) to install new hog rings. Ensure that the rear seat back cushion cover is secured to the cushion (2).
4. Install the plastic retainers which secure the seat back cushion cover to the back of the seat.
5. Install the rear seat shoulder belt guide to the rear seat back cushion.
6. Install the rear seat back cushion. Refer to Rear Split Folding Seat Back Replacement .
7. Install the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .