For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .
2. Remove the following components from the instrument panel compartment:

• | The 2 I/P compartment door hinge pins (2)

• | The I/P compartment door (1)

3. Remove the following components from the I/P compartment door, if necessary:

• | The 2 screws

• | The I/P compartment door lock

### Installation Procedure

1. Install the I/P compartment door lock to the compartment door, if removed. Secure the lock with the 2 screws.
2. Install the I/P compartment door (1) to the instrument panel compartment. Secure the door with the 2 hinge pins (2).
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .