For 1990-2009 cars

### Removal Procedure

1. Remove the rear brake shoes (6, 14). Refer to Brake Shoe Replacement .
2. Remove the wheel cylinder. Refer to Wheel Cylinder Replacement .
3. Remove the rear axle hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
4. Remove the parking brake cable from the backing plate.
5. Remove the backing plate.

### Installation Procedure

1. Install the backing plate to the vehicle.
2. Install the parking brake cable to the backing plate.
3. Install the rear axle hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
4. Install the wheel cylinder. Refer to Wheel Cylinder Replacement .
5. Install the rear brake shoes (6, 14). Refer to Brake Shoe Replacement .