For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster assembly. Refer to Instrument Cluster Replacement .
2. Remove the instrument cluster retainer (2) with the instrument cluster lens attached from the instrument cluster case (1) by releasing the 8 locking tabs.
3. Remove the instrument cluster lens (2) from the cluster retainer (1) by releasing the 8 locking tabs.

### Installation Procedure

1. Install the instrument cluster lens (2) to the instrument cluster retainer (1). Ensure that the locking tabs are fully engaged.
2. Align the cluster retainer (2) with the cluster lens attached onto the guide pins and install the retainer to the instrument cluster case (1). Ensure that the locking tabs are fully engaged.
3. Install the instrument cluster assembly. Refer to Instrument Cluster Replacement .