For 1990-2009 cars

Illustration | Tool Number/Description
--- | ---
| J 8092 Universal Driver
| J 8433 Two Jaw Puller
| J 8614-01 Flange and Pulley Holding Tool
| J 21465-13 Drive Handle Extension
| J 22912-O1 Split-Plate Bearing Puller
| J 23907 Slide Hammer with Bearing Adapter
| J 25070 Heat Gun - 500-750 F
| J 26900-12 Dial Indicator
| J 26900-13 Magnetic Indicator Base
| J 29763 Static Timing Gage
| J 36513 Gear and Bearing Separator Plate
| J 36825 Output Shaft Oil Seal Remover - 4WD Models Only
| J 36850 Transjel Lubricant
| J 44707 T Bar Push Puller
| J 44725 Gear Pack Assembly Fixture
| J 44726 2/3 Jaw Puller
| J 44728 Bearing Race Remover
| J 44730 Intermediate Case Puller Legs
| J 44731 Input Shaft Seal Installer
| J 44732 Output Shaft Seal Installer
| J 44733 Bearing Race Remover
| J 44734 Installation Aligner
| J 44735 Installation Tube
| J 44736 Bridge and Forcing Screw
| J 44737 Shift Rail Bearing Remover
| J 44738 Bearing Remover
| J 44739 Dial Indicator Bracket
| J 44741 Shift Rail Bearing Installer
| J 44742 Bearing Installer
| J 44745 Countershaft Bearing Race Installer
| J 44746 Mainshaft/Input Shaft Bearing Race Installer
| J 44749 Split Plate Bearing/Gear Puller