For 1990-2009 cars

### Removal Procedure

1. Remove the rubber boot (2) from the front door jamb switch.
2. Remove the one mounting bolt and pull the switch (1) from the door jamb.
3. Disconnect the front door jamb switch electrical connector.
4. Remove the door jamb switch (1) from the vehicle.

### Installation Procedure

1. Connect the front door jamb switch electrical connector.
2. Install the rubber boot (2) to the front door jamb switch (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the switch (1) to the door jamb. Secure the switch with the mounting bolt.

Tighten
Tighten the front door jamb switch mounting bolt to 10 N·m (89 lb in).